Electrocardiogram—change type, code N

Exported from METEOR

(AIHW's Metadata Online Registry)

© Australian Institute of Health and Welfare 2024

This product, excluding the AIHW logo, Commonwealth Coat of Arms and any material owned by a third party or protected by a trademark, has been released under a Creative Commons BY 4.0 (CC BY 4.0) licence. Excluded material owned by third parties may include, for example, design and layout, images obtained under licence from third parties and signatures. We have made all reasonable efforts to identify and label material owned by third parties.

You may distribute, remix and build on this website’s material but must attribute the AIHW as the copyright holder, in line with our attribution policy. The full terms and conditions of this licence are available at https://creativecommons.org/licenses/by/4.0/.

Enquiries relating to copyright should be addressed to info@aihw.gov.au.

Enquiries or comments on the METEOR metadata or download should be directed to the METEOR team at meteor@aihw.gov.au.

# Electrocardiogram—change type, code N

|  |
| --- |
| Identifying and definitional attributes |
| Metadata item type: | Data Element |
| Short name: | Electrocardiogram change type |
| METEOR identifier: | 356856 |
| Registration status: | [Health](https://meteor.aihw.gov.au/RegistrationAuthority/12), Standard 01/10/2008 |
| Definition: | The type of change to the heart rhythm seen on a person's electrocardiogram (ECG), as represented by a code. |
| Data Element Concept: | [Electrocardiogram—change type](https://meteor.aihw.gov.au/content/356858) |
| Value Domain: | [Electrocardiogram change type code N](https://meteor.aihw.gov.au/content/356861) |

|  |
| --- |
| Value domain attributes |
| Representational attributes |
| Representation class: | Code |
| Data type: | Number |
| Format: | NN |
| Maximum character length: | 2 |
|   | **Value** | **Meaning** |
| Permissible values: | 10 | ST-segment-elevation >= 1 mm (0.1 mV) in >= 2 contiguous limb leads |
|   | 11 | ST-segment-elevation >= 2 mm (0.2 mV) in >= 2 contiguous chest leads |
|   | 12 | ST-segment depression >= 0.5 mm (0.05 mV) in >= 2 contiguous leads (includes reciprocal changes) |
|   | 20 | T-wave inversion >= 2 mm (0.1 mV) |
|   | 30 | Significant Q waves |
|   | 40 | Left bundle-branch block (BBB) |
|   | 41 | Right bundle-branch block (BBB) |
|   | 42 | Indeterminate bundle-branch block (BBB) |
|   | 90 | Non specific |
| Supplementary values: | 99  | Not stated/inadequately described  |

|  |
| --- |
| Collection and usage attributes |
| Guide for use: | ST-segment changesCODE 10    ST-segment-elevation >= 1 mm (0.1 mV) in >= 2 contiguous limb leadsST-segment-elevation indicates greater than or equal to 1 mm (0.1 mV) elevation in 2 or more contiguous limb leads.CODE 11    ST-segment-elevation >= 2 mm (0.2 mV) in >= 2 contiguous chest leadsST-segment-elevation indicates greater than or equal to 2 mm (0.2 mV) elevation in 2 or more contiguous chest leads.CODE 12    ST-segment depression >= 0.5 mm (0.05 mV) in >= 2 contiguous leads (includes reciprocal changes)ST-segment depression of at least 0.5 mm (0.05 mV) in 2 or more contiguous leads (includes reciprocal changes).T-wave changesCODE 20     T-wave inversion >= 2 mm (0.2 mV)T-wave inversion of at least 2 mm (0.2 mV) including inverted T waves that are not indicative of acute MI.Q wave changesCODE 30    Significant Q wavesQ waves refer to the presence of Q waves that are greater than or equal to 0.03 seconds in width and greater than or equal to 1 mm (0.1 mV) in depth in at least 2 contiguous leads.Bundle-branch block changesCODE 40    Left bundle branch block (BBB)Diffuse left bundle-branch block pattern.CODE 41    Right bundle-branch block (BBB)Diffuse right bundle-branch block pattern.CODE 42    Indeterminate bundle-branch block (BBB)Bundle-branch block pattern identified, but left or right location is unclear.CODE 90    Non-specificChanges not meeting the above criteria.CODE 99    Not stated/inadequately describedIncludes unknown. |

|  |
| --- |
| Data element attributes  |
| Collection and usage attributes |
| Guide for use: | More than one code may be recorded.Record all that apply (codes 90 and 99 are excluded from multiple coding). |
| Collection methods: | Where codes 40, 41 or 42 are recorded Electrocardiogram - bundle-branch block status, code N must also be recorded. |
| Source and reference attributes |
| Submitting organisation: | Acute coronary syndrome data working group |
| Relational attributes |
| Related metadata references: | Supersedes [Person—electrocardiogram change type, code N](https://meteor.aihw.gov.au/content/285307)       [Health](https://meteor.aihw.gov.au/RegistrationAuthority/12), Superseded 01/10/2008 |
| Implementation in Data Set Specifications: | [Electrocardiogram cluster](https://meteor.aihw.gov.au/content/351884)       [Health](https://meteor.aihw.gov.au/RegistrationAuthority/12), Standard 01/10/2008***DSS specific information:*** To be provided each time an ECG is performed.  |