Device—instrumented flag, yes/no/not applicable/unknown/not stated/inadequately described code N

Exported from METEOR

(AIHW's Metadata Online Registry)

© Australian Institute of Health and Welfare 2024

This product, excluding the AIHW logo, Commonwealth Coat of Arms and any material owned by a third party or protected by a trademark, has been released under a Creative Commons BY 4.0 (CC BY 4.0) licence. Excluded material owned by third parties may include, for example, design and layout, images obtained under licence from third parties and signatures. We have made all reasonable efforts to identify and label material owned by third parties.

You may distribute, remix and build on this website’s material but must attribute the AIHW as the copyright holder, in line with our attribution policy. The full terms and conditions of this licence are available at https://creativecommons.org/licenses/by/4.0/.

Enquiries relating to copyright should be addressed to info@aihw.gov.au.

Enquiries or comments on the METEOR metadata or download should be directed to the METEOR team at meteor@aihw.gov.au.

# Device—instrumented flag, yes/no/not applicable/unknown/not stated/inadequately described code N

|  |  |
| --- | --- |
| Identifying and definitional attributes | |
| Metadata item type: | Data Element |
| Short name: | Device instrumented flag |
| METEOR identifier: | 788652 |
| Registration status: | [Australian Institute of Health and Welfare](https://meteor.aihw.gov.au/RegistrationAuthority/24), Recorded 09/02/2024 |
| Definition: | A flag of whether a device is equipped to collect, measure and or transmit data, as represented by a code. |
| Data Element Concept: | [Device—instrumented flag](https://meteor.aihw.gov.au/content/788650) |
| Value Domain: | [Yes/no/not applicable/unknown/not stated/inadequately described code N](https://meteor.aihw.gov.au/content/783859) |

|  |  |  |
| --- | --- | --- |
| Value domain attributes | | |
| Representational attributes | | |
| Representation class: | Code | |
| Data type: | Boolean | |
| Format: | N | |
| Maximum character length: | 1 | |
|  | **Value** | **Meaning** |
| Permissible values: | 1 | Yes |
|  | 2 | No |
| Supplementary values: | 7 | Not applicable |
|  | 8 | Unknown |
|  | 9 | Not stated/inadequately described |

|  |  |
| --- | --- |
| Source and reference attributes | |
| Submitting organisation: | Australian Institute of Health and Welfare |

|  |  |
| --- | --- |
| Data element attributes | |
| Collection and usage attributes | |
| Guide for use: | CODE 1     Yes  To be used when a device is equipped to collect, measure and or transmit data.  CODE 2     No  To be used when a device is not equipped to collect, measure and or transmit data.  CODE 7     Not applicable  To be used when no device is used.  CODE 8     Unknown  To be used when it is not known if a device is equipped to collect, measure and or transmit data.  CODE 9     Not stated/inadequately described  To be used when the information is not stated or otherwise inadequately described (e.g. when a response has not been recorded.) |
| Source and reference attributes | |
| Submitting organisation: | Australian Institute of Health and Welfare |
| Relational attributes | |
| Implementation in Data Set Specifications: | [Australian Sports Injury Data Dictionary](https://meteor.aihw.gov.au/content/777500)  [Australian Institute of Health and Welfare](https://meteor.aihw.gov.au/RegistrationAuthority/24), Recorded 09/08/2023  ***Conditional obligation:***  Conditional on a response being recorded for the data element [Sporting activity—protective equipment, personal code N[N]](https://meteor.aihw.gov.au/content/777259).  ***DSS specific information:***  In the ASIDD this data element collects information to flag whether the protective equipment used by the person when injured is one equipped to collect, measure and or transmit data.  One response should be recorded for every instance of the data element [Sporting activity—protective equipment, personal code N[N]](https://meteor.aihw.gov.au/content/777259). |